
**SCOPE 400 x 200 – SynthEdit1.1 Prefab**

This prefab enables monitoring the full cycle of low pitched oscillators.

It can show whole waveform of A0 note – 2 Volts in SynthEdit’s octave per volt scale.

**Inputs:**

**Signal In** – Connect a monophonic signal to be monitored.

**Pitch** – Connect a monophonic pitch signal. If you use the scope to monitor many oscillators at once, use the same pitch value as for the lowest pitched oscillator.

**GUI Controls:**

**V-Zoom** – Vertical zoom of monitored signal.

**Sample Rate** – Set it the same as sample rate of your Audio Device. Wrong sample rate settings will look like this:

